|  |  |  |
| --- | --- | --- |
| Instruction from Processing | Reply from Arduino | Example |
| get-stir | stir 1330 |  |
| get-temp | temp 20.2 |  |
| get-ph | ph 3 |  |
| set-stir 1400 | ok |  |
| set-temp 23.4 | ok |  |
| set-ph 4 | ok |  |
|  |  |  |